EMU CAF UT-440, made in Spain,
wearing the CPTM livery, 
Class 2100, Sao Paulo, Brazil
Shipped with external view for Open BVE

TECHNICAL SPECIFICATIONS: 
Continuous power: 1.160 Kw 
Maximum Speed: 130 Km/h    
Maximum acceleration: 0,40 m/s   
Height: 3,682m
Width: 2,900m
Length: 26,100m
Weights: 60.000 Kg (motor car) and 45.000 Kg (trailer car)     
Doors: 2 per side, length 2,12m each
Gauge: 1.600mm
Main frame box: carbon steel 
Power system: 3Kv VDC, overhead wires  
Operation in Brazil since 1998, renewed by Renfe and CPTM
Commom Formation: 6 cars (3 + 3)  

BVE train physics by RAFAEL SANTELLO
gospelrafa@yahoo.com.br
www.paodavida.cjb.net

Sounds, panel and textures by 
ALEXANDRE BEZERRA BARBOSA

3-D assembling and hosting by Joao Carlos Goncalves
http://www.bvebrasil.com.br
joaocg@iconet.com.br